|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| BEL-Logo-PNG | ACCEPTANCE TEST PROCEDURE | | | DOC CODE  ATP |  | |
|
|
|
| QSRx with SFBs |  |  |  |  |  |  |
|  |  |
|  |  |  |  |  |  |
|  |  |

Test Data Records

Sl. No. Date:

Test Condition:

Test: SFB2 - Amplitude & Phase Tracking Measurement 1GHz IF

I/P Power: -20 dBm

Port: BITE

|  |  |  |  |
| --- | --- | --- | --- |
| Band | Frequency (GHz) | Amplitude Tracking (Db) | Phase Tracking (deg) |
| 1 | 2.0 - 2.75 | 0 | 0 |
| 2 | 2.5 - 3.75 | 0 | 0 |
| 3 | 3.5 - 5.25 | 0 | 0 |
| 4 | 5.0 - 6.25 | 0 | 0 |

RESULT : OK/NOT OK

**REP. BEL REP.CQAE(N)**